MERCURY MARINE

DIVISION OF BRUNSWICK CORP.

FOND DU LAC, WIS. 54935 U.S.A.

OPERATION

1. USE RECOMMENDED GASOLINES AND OILS.
2. OPEN TANK VENT.
3. CONNECT FUEL LINE AND PRIME WITH BULB.
4. PLACE SHIFT LEVER IN NEUTRAL.
5. PLACE THROTTLE IN START POSITION.

SERIAL NO.

1. PULL STARTER ROPE, IF MOTOR IS COLD  
   USE CHOKE.
2. PRESS STOP BUTTON OR CHOKE TO STOP.
3. SHIFT GEARS ONLY WITH MOTOR RUNNING.
4. DISCONNECT FUEL LINE WHEN NOT IN USE.