Albert’s 390 Express Cruiser.

Generator Start Procedure

1. Open water intake seacock
2. Check Oil Level, belts, hoses, coolant. Fluids in pan under generator.
3. Set RUN switch to RUN on remote panel
4. Hold Preheat switch on for 20 seconds
5. Hold START switch on until generator starts. Hold Preheat switch on for an additional 10 to 20 seconds to allow oil pressure to come up and allow fuel solenoid valve to remain open.

Engine Start Procedure

1. Open water intake sea cocks.
2. Check for debris in strainer and/ or sea water leaks.
3. Check engine oil level and transmission oil levels. Check for evidence of fluids in pan below engine and transmission. If fluids are present determine why.
4. Check alternator and sea water pump belts.
5. Check Coolant levels. Finger should be able to touch coolant with cap removed. DO NOT OPEN WHEN ENGINE IS HOT!!
6. Turn on ignition breakers.
7. Set throttle levers (Red Handles) all the way aft.
8. Set gear shift handles (Black Handles) to neutral marks in middle of base plate. Engine will not crank unless gear shift is in NEUTRAL.
9. Turn key switch clockwise to crank and start engine. Release key when engine starts.

Prior to getting under way

1. Turn on the following breaker switches
(Port switch bank)
Trim Tabs
(Starboard switch bank)
Acc
Horn
Wipers
Bilge Pump switches should remain in center position for automatic operation.
2. Turn on navigation multi function display. Engage chart plotter and radar as necessary.
3. Turn on VHF radio and set to channel 16 monitoring.